2. REGISTER sip:46.101.55.90 SIP/2.0

Via: SIP/2.0/UDP 192.168.1.46:54550;branch=z9hG4bK-524287-1---b6b2c75479158243;rport

Max-Forwards: 70

Contact: <sip:1000@192.168.1.46:54550;rinstance=40a63c84743b74de>

To: "1000"<sip:1000@46.101.55.90>

From: "1000"<sip:1000@46.101.55.90>;tag=bd987919

Call-ID: 76464NjdmZjYxMTc1ZWY1NWU0NDMyM2ZlZTVlNzVlM2ZkNjg

CSeq: 1 REGISTER

Expires: 3600

Allow: SUBSCRIBE, NOTIFY, INVITE, ACK, CANCEL, BYE, REFER, INFO, MESSAGE

User-Agent: X-Lite 4.8.3 76464-d355af21-W6.1

Content-Length: 0

SIP/2.0 200 OK

Via: SIP/2.0/UDP 192.168.1.46:54550;branch=z9hG4bK-524287-1---b6b2c75479158243;rport=2090;received=83.220.51.235

To: "1000"<sip:1000@46.101.55.90>;tag=c97b4d1cb1f3d0da549e06a8d482ef63.8006

From: "1000"<sip:1000@46.101.55.90>;tag=bd987919

Call-ID: 76464NjdmZjYxMTc1ZWY1NWU0NDMyM2ZlZTVlNzVlM2ZkNjg

CSeq: 1 REGISTER

Contact: <sip:1000@192.168.1.46:19926;rinstance=1a5a0966392d6b04>;expires=3138, <sip:1000@192.168.1.46:54550;rinstance=40a63c84743b74de>;expires=3600

Server: OpenSIPS (1.5.3-notls (i386/linux))

Content-Length: 0

3. REGISTER sip:46.101.55.90 SIP/2.0

Via: SIP/2.0/UDP 192.168.1.46:54550;branch=z9hG4bK-524287-1---5782217eec54a33d;rport

Max-Forwards: 70

Contact: <sip:1000@192.168.1.46:54550;rinstance=40a63c84743b74de>;expires=0

To: "1000"<sip:1000@46.101.55.90>

From: "1000"<sip:1000@46.101.55.90>;tag=bd987919

Call-ID: 76464NjdmZjYxMTc1ZWY1NWU0NDMyM2ZlZTVlNzVlM2ZkNjg

CSeq: 2 REGISTER

Allow: SUBSCRIBE, NOTIFY, INVITE, ACK, CANCEL, BYE, REFER, INFO, MESSAGE

User-Agent: X-Lite 4.8.3 76464-d355af21-W6.1

Content-Length: 0

SIP/2.0 200 OK

Via: SIP/2.0/UDP 192.168.1.46:54550;branch=z9hG4bK-524287-1---5782217eec54a33d;rport=2090;received=83.220.51.235

To: "1000"<sip:1000@46.101.55.90>;tag=c97b4d1cb1f3d0da549e06a8d482ef63.73cb

From: "1000"<sip:1000@46.101.55.90>;tag=bd987919

Call-ID: 76464NjdmZjYxMTc1ZWY1NWU0NDMyM2ZlZTVlNzVlM2ZkNjg

CSeq: 2 REGISTER

Contact: <sip:1000@192.168.1.46:19926;rinstance=1a5a0966392d6b04>;expires=3138

Server: OpenSIPS (1.5.3-notls (i386/linux))

Content-Length: 0

4. REGISTER sip:46.101.55.90 SIP/2.0

Via: SIP/2.0/UDP 192.168.1.46:54550;branch=z9hG4bK-524287-1---f27e9465a16b6761;rport

Max-Forwards: 70

Contact: <sip:1000@83.220.51.235:2090;rinstance=c953b71647d0fa66>

To: "1000"<sip:1000@46.101.55.90>

From: "1000"<sip:1000@46.101.55.90>;tag=bd987919

Call-ID: 76464NjdmZjYxMTc1ZWY1NWU0NDMyM2ZlZTVlNzVlM2ZkNjg

CSeq: 3 REGISTER

Expires: 3600

Allow: SUBSCRIBE, NOTIFY, INVITE, ACK, CANCEL, BYE, REFER, INFO, MESSAGE

User-Agent: X-Lite 4.8.3 76464-d355af21-W6.1

Content-Length: 0

SIP/2.0 200 OK

Via: SIP/2.0/UDP 192.168.1.46:54550;branch=z9hG4bK-524287-1---f27e9465a16b6761;rport=2090;received=83.220.51.235

To: "1000"<sip:1000@46.101.55.90>;tag=c97b4d1cb1f3d0da549e06a8d482ef63.4d7f

From: "1000"<sip:1000@46.101.55.90>;tag=bd987919

Call-ID: 76464NjdmZjYxMTc1ZWY1NWU0NDMyM2ZlZTVlNzVlM2ZkNjg

CSeq: 3 REGISTER

Contact: <sip:1000@192.168.1.46:19926;rinstance=1a5a0966392d6b04>;expires=3138, <sip:1000@83.220.51.235:2090;rinstance=c953b71647d0fa66>;expires=3600

Server: OpenSIPS (1.5.3-notls (i386/linux))

Content-Length: 0

5. SUBSCRIBE sip:1000@46.101.55.90 SIP/2.0

Via: SIP/2.0/UDP 192.168.1.46:54550;branch=z9hG4bK-524287-1---04f0f37143d74229;rport

Max-Forwards: 70

Contact: <sip:1000@83.220.51.235:2090;rinstance=c953b71647d0fa66>

To: <sip:1000@46.101.55.90>

From: "1000"<sip:1000@46.101.55.90>;tag=123dc201

Call-ID: 76464ZTllMzVmZWExMzEyZGY3ZDgwNDZiYTFiZmQ4MGQ0OTk

CSeq: 1 SUBSCRIBE

Expires: 300

Accept: application/simple-message-summary

Allow: SUBSCRIBE, NOTIFY, INVITE, ACK, CANCEL, BYE, REFER, INFO, MESSAGE

User-Agent: X-Lite 4.8.3 76464-d355af21-W6.1

Event: message-summary

Content-Length: 0

SUBSCRIBE sip:1000@83.220.51.235:2090;rinstance=c953b71647d0fa66 SIP/2.0

Record-Route: <sip:46.101.55.90;lr=on>

Via: SIP/2.0/UDP 46.101.55.90;branch=z9hG4bK9cc3.6d993cd5.1

Via: SIP/2.0/UDP 192.168.1.46:54550;received=83.220.51.235;branch=z9hG4bK-524287-1---04f0f37143d74229;rport=2090

Max-Forwards: 69

Contact: <sip:1000@83.220.51.235:2090;rinstance=c953b71647d0fa66>

To: <sip:1000@46.101.55.90>

From: "1000"<sip:1000@46.101.55.90>;tag=123dc201

Call-ID: 76464ZTllMzVmZWExMzEyZGY3ZDgwNDZiYTFiZmQ4MGQ0OTk

CSeq: 1 SUBSCRIBE

Expires: 300

Accept: application/simple-message-summary

Allow: SUBSCRIBE, NOTIFY, INVITE, ACK, CANCEL, BYE, REFER, INFO, MESSAGE

User-Agent: X-Lite 4.8.3 76464-d355af21-W6.1

Event: message-summary

Content-Length: 0

6. SIP/2.0 489 Event Package Not Supported

Via: SIP/2.0/UDP 46.101.55.90;branch=z9hG4bK9cc3.6d993cd5.1

Via: SIP/2.0/UDP 192.168.1.46:54550;received=83.220.51.235;branch=z9hG4bK-524287-1---04f0f37143d74229;rport=2090

To: <sip:1000@46.101.55.90>;tag=33fd6077

From: "1000"<sip:1000@46.101.55.90>;tag=123dc201

Call-ID: 76464ZTllMzVmZWExMzEyZGY3ZDgwNDZiYTFiZmQ4MGQ0OTk

CSeq: 1 SUBSCRIBE

User-Agent: X-Lite release 4.8.3 stamp 76464

Content-Length: 0